SHORT L2 cache bandwidth in MBytes/s

EVENTSET
PMC0  DATA_CACHE_REFILLS_ALL
PMC1  DATA_CACHE_REFILLS_SYSTEM
PMC2  CPU_CLOCKS_UNHALTED

METRICS
Runtime (RDTSC) [s] time
L2 bandwidth [MBytes/s]   1.0E-06*(PMC0-PMC1)*64.0/time
L2 data volume [GBytes]   1.0E-09*(PMC0-PMC1)*64.0
Cache refill bandwidth System/L2 [MBytes/s]   1.0E-06*PMC0*64.0/time
Cache refill bandwidth System  [MBytes/s]    1.0E-06*PMC1*64.0/time

LONG
Formulas:
L2 bandwidth [MBytes/s]   1.0E-06*(DATA_CACHE_REFILLS_ALL-DATA_CACHE_REFILLS_SYSTEM)*64/time
L2 data volume [GBytes]   1.0E-09*(DATA_CACHE_REFILLS_ALL-DATA_CACHE_REFILLS_SYSTEM)*64
Cache refill bandwidth system/L2 [MBytes/s]   1.0E-06*DATA_CACHE_REFILLS_ALL*64/time
Cache refill bandwidth system [MBytes/s]   1.0E-06*DATA_CACHE_REFILLS_SYSTEM*64/time
-
Profiling group to measure L2 cache bandwidth. The bandwidth is
computed by the number of cache line loaded from L2 to L1 and the
number of modified cache lines evicted from the L1.
Note that this bandwidth also included data transfers due to a
write allocate load on a store miss in L1 and copy back transfers if
originated from L2. L2-L2 data volume is the total data volume transferred
between L2 and L1.

