SHORT Cache and memory bandwidths

EVENTSET
PMC0  L1D_REPLACEMENT
PMC1  L2_TRANS_L1D_WB
PMC2  L2_LINES_IN_ALL
PMC3  L2_LINES_OUT_DEMAND_DIRTY

METRICS
SUM L2 bandwidth [MBytes/s] 1.0E-06*(PMC0+PMC1)*64.0/time
SUM L3 bandwidth [MBytes/s] 1.0E-06*(PMC2+PMC3)*64.0/time

LONG
