SHORT Load to store ratio

EVENTSET
FIXC0 INSTR_RETIRED_ANY
FIXC1 CPU_CLK_UNHALTED_CORE
FIXC2 CPU_CLK_UNHALTED_REF
PMC0  MEM_UOPS_RETIRED_LOADS
PMC1  MEM_UOPS_RETIRED_STORES
PMC2  UOPS_RETIRED_ALL

METRICS
Runtime (RDTSC) [s] time
Runtime unhalted [s] FIXC1*inverseClock
Clock [MHz]  1.E-06*(FIXC1/FIXC2)/inverseClock
CPI  FIXC1/FIXC0
Load to store ratio PMC0/PMC1
Load ratio PMC0/PMC2
Store ratio PMC1/PMC2

LONG
Formulas:
Load to store ratio = MEM_UOPS_RETIRED_LOADS/MEM_UOPS_RETIRED_STORES
Load ratio = MEM_UOPS_RETIRED_LOADS/UOPS_RETIRED_ALL
Store ratio = MEM_UOPS_RETIRED_STORES/UOPS_RETIRED_ALL
-
This is a metric to determine your load to store ratio.

