SHORT Main memory bandwidth in MBytes/s

EVENTSET
FIXC0   INSTR_RETIRED_ANY
FIXC1   CPU_CLK_UNHALTED_CORE
FIXC2   CPU_CLK_UNHALTED_REF
MBOX0C0 CAS_COUNT_RD
MBOX0C1 CAS_COUNT_WR
MBOX1C0 CAS_COUNT_RD
MBOX1C1 CAS_COUNT_WR
MBOX2C0 CAS_COUNT_RD
MBOX2C1 CAS_COUNT_WR
MBOX3C0 CAS_COUNT_RD
MBOX3C1 CAS_COUNT_WR

METRICS
Runtime (RDTSC) [s] time
Runtime unhalted [s] FIXC1*inverseClock
Clock [MHz]  1.E-06*(FIXC1/FIXC2)/inverseClock
CPI  FIXC1/FIXC0
Memory read bandwidth [MBytes/s] 1.0E-06*(MBOX0C0+MBOX1C0+MBOX2C0+MBOX3C0)*64.0/time
Memory read data volume [GBytes] 1.0E-09*(MBOX0C0+MBOX1C0+MBOX2C0+MBOX3C0)*64.0
Memory write bandwidth [MBytes/s] 1.0E-06*(MBOX0C1+MBOX1C1+MBOX2C1+MBOX3C1)*64.0/time
Memory write data volume [GBytes] 1.0E-09*(MBOX0C1+MBOX1C1+MBOX2C1+MBOX3C1)*64.0
Memory bandwidth [MBytes/s] 1.0E-06*(MBOX0C0+MBOX1C0+MBOX2C0+MBOX3C0+MBOX0C1+MBOX1C1+MBOX2C1+MBOX3C1)*64.0/time
Memory data volume [GBytes] 1.0E-09*(MBOX0C0+MBOX1C0+MBOX2C0+MBOX3C0+MBOX0C1+MBOX1C1+MBOX2C1+MBOX3C1)*64.0

LONG
Formulas:
Memory read bandwidth [MBytes/s] = 1.0E-06*(SUM(MBOXxC0))*64.0/time
Memory read data volume [GBytes] = 1.0E-09*(SUM(MBOXxC0))*64.0
Memory write bandwidth [MBytes/s] = 1.0E-06*(SUM(MBOXxC1))*64.0/time
Memory write data volume [GBytes] = 1.0E-09*(SUM(MBOXxC1))*64.0
Memory bandwidth [MBytes/s] = 1.0E-06*(SUM(MBOXxC0)+SUM(MBOXxC1))*64.0/time
Memory data volume [GBytes] = 1.0E-09*(SUM(MBOXxC0)+SUM(MBOXxC1))*64.0
-
Profiling group to measure memory bandwidth drawn by all cores of a socket.
Since this group is based on Uncore events it is only possible to measure on a
per socket base. Also outputs total data volume transferred from main memory.

