SHORT UOPs issueing

EVENTSET
FIXC0 INSTR_RETIRED_ANY
FIXC1 CPU_CLK_UNHALTED_CORE
FIXC2 CPU_CLK_UNHALTED_REF
PMC0  UOPS_ISSUED_USED_CYCLES
PMC1  UOPS_ISSUED_STALL_CYCLES
PMC2  CPU_CLOCK_UNHALTED_TOTAL_CYCLES
PMC3:EDGEDETECT  UOPS_ISSUED_STALL_CYCLES

METRICS
Runtime (RDTSC) [s] time
Runtime unhalted [s] FIXC1*inverseClock
Clock [MHz]  1.E-06*(FIXC1/FIXC2)/inverseClock
CPI  FIXC1/FIXC0
Used cycles ratio [%] 100*PMC0/PMC2
Unused cycles ratio [%] 100*PMC1/PMC2
Avg stall duration [cycles] PMC1/PMC3:EDGEDETECT


LONG
Formulas:
Used cycles ratio [%] = 100*UOPS_ISSUED_USED_CYCLES/CPU_CLK_UNHALTED_CORE
Unused cycles ratio [%] = 100*UOPS_ISSUED_STALL_CYCLES/CPU_CLK_UNHALTED_CORE
Avg stall duration [cycles] = UOPS_ISSUED_STALL_CYCLES/UOPS_ISSUED_STALL_CYCLES:EDGEDETECT
-
This performance group returns the ratios of used and unused cycles regarding
the issue stage in the pipeline. Used cycles are all cycles where uOPs are
issued while unused cycles refer to pipeline stalls. Moreover, the group
calculates the average stall duration in cycles.
