SHORT Overview of arithmetic and main memory performance

EVENTSET
FIXC0 INSTR_RETIRED_ANY
FIXC1 CPU_CLK_UNHALTED_CORE
FIXC2 CPU_CLK_UNHALTED_REF
PWR0  PWR_PKG_ENERGY
PWR3  PWR_DRAM_ENERGY
PMC0  FP_ARITH_INST_RETIRED_128B_PACKED_DOUBLE
PMC1  FP_ARITH_INST_RETIRED_SCALAR_DOUBLE
PMC2  FP_ARITH_INST_RETIRED_256B_PACKED_DOUBLE
MBOX0C0 CAS_COUNT_RD
MBOX0C1 CAS_COUNT_WR
MBOX1C0 CAS_COUNT_RD
MBOX1C1 CAS_COUNT_WR
MBOX2C0 CAS_COUNT_RD
MBOX2C1 CAS_COUNT_WR
MBOX3C0 CAS_COUNT_RD
MBOX3C1 CAS_COUNT_WR
MBOX4C0 CAS_COUNT_RD
MBOX4C1 CAS_COUNT_WR
MBOX5C0 CAS_COUNT_RD
MBOX5C1 CAS_COUNT_WR
MBOX6C0 CAS_COUNT_RD
MBOX6C1 CAS_COUNT_WR
MBOX7C0 CAS_COUNT_RD
MBOX7C1 CAS_COUNT_WR

METRICS
Runtime (RDTSC) [s] time
Runtime unhalted [s] FIXC1*inverseClock
Clock [MHz]  1.E-06*(FIXC1/FIXC2)/inverseClock
CPI  FIXC1/FIXC0
Energy [J]  PWR0
Power [W] PWR0/time
Energy DRAM [J]  PWR3
Power DRAM [W] PWR3/time
MFLOP/s  1.0E-06*(PMC0*2.0+PMC1+PMC2*4.0)/time
AVX MFLOP/s  1.0E-06*(PMC2*4.0)/time
Packed MUOPS/s   1.0E-06*(PMC0+PMC2)/time
Scalar MUOPS/s 1.0E-06*PMC1/time
Memory read bandwidth [MBytes/s] 1.0E-06*(MBOX0C0+MBOX1C0+MBOX2C0+MBOX3C0+MBOX4C0+MBOX5C0+MBOX6C0+MBOX7C0)*64.0/time
Memory read data volume [GBytes] 1.0E-09*(MBOX0C0+MBOX1C0+MBOX2C0+MBOX3C0+MBOX4C0+MBOX5C0+MBOX6C0+MBOX7C0)*64.0
Memory write bandwidth [MBytes/s] 1.0E-06*(MBOX0C1+MBOX1C1+MBOX2C1+MBOX3C1+MBOX4C1+MBOX5C1+MBOX6C1+MBOX7C1)*64.0/time
Memory write data volume [GBytes] 1.0E-09*(MBOX0C1+MBOX1C1+MBOX2C1+MBOX3C1+MBOX4C1+MBOX5C1+MBOX6C1+MBOX7C1)*64.0
Memory bandwidth [MBytes/s] 1.0E-06*(MBOX0C0+MBOX1C0+MBOX2C0+MBOX3C0+MBOX4C0+MBOX5C0+MBOX6C0+MBOX7C0+MBOX0C1+MBOX1C1+MBOX2C1+MBOX3C1+MBOX4C1+MBOX5C1+MBOX6C1+MBOX7C1)*64.0/time
Memory data volume [GBytes] 1.0E-09*(MBOX0C0+MBOX1C0+MBOX2C0+MBOX3C0+MBOX4C0+MBOX5C0+MBOX6C0+MBOX7C0+MBOX0C1+MBOX1C1+MBOX2C1+MBOX3C1+MBOX4C1+MBOX5C1+MBOX6C1+MBOX7C1)*64.0

LONG
Formula:
MFLOP/s = 1.0E-06*(FP_ARITH_INST_RETIRED_128B_PACKED_DOUBLE*2+FP_ARITH_INST_RETIRED_SCALAR_DOUBLE+FP_ARITH_INST_RETIRED_256B_PACKED_DOUBLE*4)/runtime
AVX MFLOP/s = 1.0E-06*(FP_ARITH_INST_RETIRED_256B_PACKED_DOUBLE*4)/runtime
Packed MUOPS/s = 1.0E-06*(FP_ARITH_INST_RETIRED_128B_PACKED_DOUBLE+FP_ARITH_INST_RETIRED_256B_PACKED_DOUBLE)/runtime
Scalar MUOPS/s = 1.0E-06*FP_ARITH_INST_RETIRED_SCALAR_DOUBLE/runtime
Memory read bandwidth [MBytes/s] = 1.0E-06*(SUM(MBOXxC0))*64.0/runtime
Memory read data volume [GBytes] = 1.0E-09*(SUM(MBOXxC0))*64.0
Memory write bandwidth [MBytes/s] = 1.0E-06*(SUM(MBOXxC1))*64.0/runtime
Memory write data volume [GBytes] = 1.0E-09*(SUM(MBOXxC1))*64.0
Memory bandwidth [MBytes/s] = 1.0E-06*(SUM(MBOXxC0)+SUM(MBOXxC1))*64.0/runtime
Memory data volume [GBytes] = 1.0E-09*(SUM(MBOXxC0)+SUM(MBOXxC1))*64.0
--
Profiling group to measure memory bandwidth drawn by all cores of a socket.
Since this group is based on Uncore events it is only possible to measure on
a per socket base. Also outputs total data volume transferred from main memory.
SSE scalar and packed double precision FLOP rates. Also reports on packed AVX
32b instructions.
