SHORT Local and remote memory accesses

EVENTSET
FIXC0 INSTR_RETIRED_ANY
FIXC1 CPU_CLK_UNHALTED_CORE
FIXC2 CPU_CLK_UNHALTED_REF
PMC0 OFFCORE_RESPONSE_0_LOCAL_DRAM
PMC1 OFFCORE_RESPONSE_1_REMOTE_DRAM

METRICS
Runtime (RDTSC) [s] time
Runtime unhalted [s] FIXC1*inverseClock
Clock [MHz]  1.E-06*(FIXC1/FIXC2)/inverseClock
CPI  FIXC1/FIXC0
Local DRAM data volume [GByte]  1.E-09*PMC0*64
Local DRAM bandwidth [MByte/s]  1.E-06*(PMC0*64)/time
Remote DRAM data volume [GByte]  1.E-09*PMC1*64
Remote DRAM bandwidth [MByte/s]  1.E-06*(PMC1*64)/time
Memory data volume [GByte]  1.E-09*(PMC0+PMC1)*64
Memory bandwidth [MByte/s]  1.E-06*((PMC0+PMC1)*64)/time

LONG
Formula:
CPI = CPU_CLK_UNHALTED_CORE/INSTR_RETIRED_ANY
Local DRAM data volume [GByte] = 1.E-09*OFFCORE_RESPONSE_0_LOCAL_DRAM*64
Local DRAM bandwidth [MByte/s] = 1.E-06*(OFFCORE_RESPONSE_0_LOCAL_DRAM*64)/time
Remote DRAM data volume [GByte] = 1.E-09*OFFCORE_RESPONSE_1_REMOTE_DRAM*64
Remote DRAM bandwidth [MByte/s] = 1.E-06*(OFFCORE_RESPONSE_1_REMOTE_DRAM*64)/time
Memory data volume [GByte] = 1.E-09*(OFFCORE_RESPONSE_0_LOCAL_DRAM+OFFCORE_RESPONSE_1_REMOTE_DRAM)*64
Memory bandwidth [MByte/s] = 1.E-06*((OFFCORE_RESPONSE_0_LOCAL_DRAM+OFFCORE_RESPONSE_1_REMOTE_DRAM)*64)/time
--
This performance group measures the data traffic of CPU cores to local and remote
memory.
