SHORT Cache and memory bandwidths

EVENTSET
PMC0  DATA_CACHE_REFILLS_ALL
PMC1  DATA_CACHE_REFILLS_SYSTEM
PMC2  L2_FILL_WB_FILL
PMC3  L2_FILL_WB_WB
UPMC0  UNC_DRAM_ACCESSES_DCT0_ALL
UPMC1  UNC_DRAM_ACCESSES_DCT1_ALL

METRICS
SUM L2 bandwidth [MBytes/s] 1.0E-06*(PMC0-PMC1)*64.0/time
SUM L3 bandwidth [MBytes/s] 1.0E-06*(PMC2+PMC3)*64.0/time
SUM Memory bandwidth [MBytes/s] 1.0E-06*(UPMC0+UPMC1)*64.0/time

LONG
