SHORT  Instruction cache miss rate/ratio

EVENTSET
FIXC0 INSTR_RETIRED_ANY
FIXC1 CPU_CLK_UNHALTED_CORE
FIXC2 CPU_CLK_UNHALTED_REF
PMC0  L1I_READS
PMC1  L1I_MISSES

METRICS
Runtime (RDTSC) [s] time
Runtime unhalted [s] FIXC1*inverseClock
Clock [MHz]  1.E-06*(FIXC1/FIXC2)/inverseClock
CPI  FIXC1/FIXC0
L1I request rate PMC0/FIXC0
L1I miss rate PMC1/FIXC0
L1I miss ratio PMC1/PMC0

LONG
Formulas:
L1I request rate = L1I_READS / INSTR_RETIRED_ANY
L1I miss rate = ICACHE_MISSES / INSTR_RETIRED_ANY
L1I miss ratio = ICACHE_MISSES / L1I_READS
-
This group measures some L1 instruction cache metrics.
