SHORT UOPs execution info

EVENTSET
FIXC0 INSTR_RETIRED_ANY
FIXC1 CPU_CLK_UNHALTED_CORE
FIXC2 CPU_CLK_UNHALTED_REF
PMC0  UOPS_ISSUED_ANY
PMC1  UOPS_EXECUTED_THREAD
PMC2  UOPS_RETIRED_ALL
PMC3  UOPS_ISSUED_FUSED



METRICS
Runtime (RDTSC) [s] time
Runtime unhalted [s] FIXC1*inverseClock
Clock [MHz]  1.E-06*(FIXC1/FIXC2)/inverseClock
CPI  FIXC1/FIXC0
Issued UOPs PMC0
Merged UOPs PMC3
Executed UOPs PMC1
Retired UOPs PMC2

LONG
Formula:
Issued UOPs = UOPS_ISSUED_ANY
Merged UOPs = UOPS_ISSUED_FUSED
Executed UOPs = UOPS_EXECUTED_THREAD
Retired UOPs = UOPS_RETIRED_ALL
-
This group returns information about the instruction pipeline. It measures the
issued, executed and retired uOPs and returns the number of uOPs which were issued
but not executed as well as the number of uOPs which were executed but never retired.
The executed but not retired uOPs commonly come from speculatively executed branches.

