SHORT L2 cache bandwidth in MBytes/s

EVENTSET
PMC0  DATA_CACHE_REFILLS_ALL
PMC1  DATA_CACHE_EVICTED_ALL
PMC2  CPU_CLOCKS_UNHALTED

METRICS
Runtime (RDTSC) [s] time
Runtime unhalted [s]   PMC2*inverseClock
L2D load bandwidth [MBytes/s]  1.0E-06*PMC0*64.0/time
L2D load data volume [GBytes]  1.0E-09*PMC0*64.0
L2D evict bandwidth [MBytes/s]  1.0E-06*PMC1*64.0/time
L2D evict data volume [GBytes]  1.0E-09*PMC1*64.0
L2 bandwidth [MBytes/s]   1.0E-06*(PMC0+PMC1)*64.0/time
L2 data volume [GBytes]   1.0E-09*(PMC0+PMC1)*64.0

LONG
Formulas:
L2D load bandwidth [MBytes/s] = 1.0E-06*DATA_CACHE_REFILLS_ALL*64.0/time
L2D load data volume [GBytes] = 1.0E-09*DATA_CACHE_REFILLS_ALL*64.0
L2D evict bandwidth [MBytes/s] = 1.0E-06*DATA_CACHE_EVICTED_ALL*64.0/time
L2D evict data volume [GBytes] = 1.0E-09*DATA_CACHE_EVICTED_ALL*64.0
L2 bandwidth [MBytes/s] = 1.0E-06*(DATA_CACHE_REFILLS_ALL+DATA_CACHE_EVICTED_ALL)*64/time
L2 data volume [GBytes] = 1.0E-09*(DATA_CACHE_REFILLS_ALL+DATA_CACHE_EVICTED_ALL)*64
-
Profiling group to measure L2 cache bandwidth. The bandwidth is
computed by the number of cache line loaded from L2 to L1 and the
number of modified cache lines evicted from the L1.
Note that this bandwidth also includes data transfers due to a
write allocate load on a store miss in L1 and copy back transfers if
originated from L2.

