SHORT Memory load bandwidth in MBytes/s

EVENTSET
FIXC0 INSTR_RETIRED_ANY
FIXC1 CPU_CLK_UNHALTED_CORE
FIXC2 CPU_CLK_UNHALTED_REF
PMC0  LONGEST_LAT_CACHE_MISS
PMC1  OFFCORE_RESPONSE_1_WB_ANY

METRICS
Runtime (RDTSC) [s] time
Runtime unhalted [s] FIXC1*inverseClock
Clock [MHz]  1.E-06*(FIXC1/FIXC2)/inverseClock
CPI  FIXC1/FIXC0
Memory read bandwidth [MBytes/s] 1.0E-06*(PMC0)*64.0/time
Memory read data volume [GBytes] 1.0E-09*(PMC0)*64.0
Memory writeback bandwidth [MBytes/s] 1.0E-06*(PMC1)*64.0/time
Memory writeback data volume [GBytes] 1.0E-09*(PMC1)*64.0
Memory bandwidth [MBytes/s] 1.0E-06*(PMC0+PMC1)*64.0/time
Memory data volume [GBytes] 1.0E-09*(PMC0+PMC1)*64.0

LONG
Formulas:
Memory read bandwidth [MBytes/s] = 1.0E-06*(LONGEST_LAT_CACHE_MISS)*64/time
Memory read data volume [GBytes] = 1.0E-09*(LONGEST_LAT_CACHE_MISS)*64
Memory writeback bandwidth [MBytes/s] = 1.0E-06*(OFFCORE_RESPONSE_1_WB_ANY)*64/time
Memory writeback data volume [GBytes] = 1.0E-09*(OFFCORE_RESPONSE_1_WB_ANY)*64
Memory bandwidth [MBytes/s] = 1.0E-06*(LONGEST_LAT_CACHE_MISS+OFFCORE_RESPONSE_1_WB_ANY)*64/time
Memory data volume [GBytes] = 1.0E-09*(LONGEST_LAT_CACHE_MISS+OFFCORE_RESPONSE_1_WB_ANY)*64
-
Profiling group to measure L2 to MEM load cache bandwidth. The bandwidth is computed by the
number of cache line allocated in the L2 cache. Since there is no possibility to retrieve
the evicted cache lines, this group measures only the load cache bandwidth. The
writeback metrics count only modified cache lines that are written back to go to
exclusive state
The group also output totally load and writeback data volume transferred between memory and L2.

