SHORT Single Precision MFlops/s

EVENTSET
PMC0  FP_ARITH_INST_RETIRED_128B_PACKED_SINGLE
PMC1  FP_ARITH_INST_RETIRED_SCALAR_SINGLE
PMC2  FP_ARITH_INST_RETIRED_256B_PACKED_SINGLE

METRICS
MFlops/s  1.0E-06*(PMC0*4.0+PMC1+PMC2*8.0)/time
AVX MFlops/s  1.0E-06*(PMC2*8.0)/time
Packed MUOPS/s   1.0E-06*(PMC0+PMC2)/time
Scalar MUOPS/s 1.0E-06*PMC1/time

LONG
Formula:
MFlops/s = 1.0E-06*(FP_ARITH_INST_RETIRED_128B_PACKED_SINGLE*4+FP_ARITH_INST_RETIRED_SCALAR_SINGLE+FP_ARITH_INST_RETIRED_256B_PACKED_SINGLE*8)/runtime
AVX MFlops/s = 1.0E-06*(FP_ARITH_INST_RETIRED_256B_PACKED_SINGLE*8)/runtime
Packed MUOPS/s = 1.0E-06*(FP_ARITH_INST_RETIRED_128B_PACKED_SINGLE+FP_ARITH_INST_RETIRED_256B_PACKED_SINGLE)/runtime
Scalar MUOPS/s = 1.0E-06*FP_ARITH_INST_RETIRED_SCALAR_SINGLE/runtime
-
AVX/SSE scalar and packed single precision flop rates.

