SHORT L2 cache bandwidth in MBytes/s

EVENTSET
FIXC0 INSTR_RETIRED_ANY
FIXC1 CPU_CLK_UNHALTED_CORE
FIXC2 CPU_CLK_UNHALTED_REF
PMC0  L1D_REPL
PMC1  L1D_M_EVICT
PMC2  L1I_MISSES

METRICS
Runtime (RDTSC) [s] time
Runtime unhalted [s] FIXC1*inverseClock
Clock [MHz]  1.E-06*(FIXC1/FIXC2)/inverseClock
CPI  FIXC1/FIXC0
L2D load bandwidth [MBytes/s]  1.0E-06*PMC0*64.0/time
L2D load data volume [GBytes]  1.0E-09*PMC0*64.0
L2D evict bandwidth [MBytes/s]  1.0E-06*PMC1*64.0/time
L2D evict data volume [GBytes]  1.0E-09*PMC1*64.0
L2 bandwidth [MBytes/s] 1.0E-06*(PMC0+PMC1+PMC2)*64.0/time
L2 data volume [GBytes] 1.0E-09*(PMC0+PMC1+PMC2)*64.0

LONG
Formulas:
L2D load bandwidth [MBytes/s] = 1.0E-06*L1D_REPL*64.0/time
L2D load data volume [GBytes] = 1.0E-09*L1D_REPL*64.0
L2D evict bandwidth [MBytes/s] = 1.0E-06*L1D_M_EVICT*64.0/time
L2D evict data volume [GBytes] = 1.0E-09*L1D_M_EVICT*64.0
L2 bandwidth [MBytes/s] = 1.0E-06*(L1D_REPL+L1D_M_EVICT+L1I_MISSES)*64/time
L2 data volume [GBytes] = 1.0E-09*(L1D_REPL+L1D_M_EVICT+L1I_MISSES)*64
-
Profiling group to measure L2 cache bandwidth. The bandwidth is computed by the
number of cache line allocated in the L1 and the number of modified cache lines
evicted from the L1. The group also reports of data volume transferred between
L2 and L1 cache. Note that this bandwidth also includes data transfers due to a
write allocate load on a store miss in L1 and traffic caused by misses in the
L1 instruction cache.

