SHORT HW prefetch transfers

EVENTSET
PMC0  HWP_L2MISS

METRICS
Runtime (RDTSC) [s] time
Prefetch bandwidth [MBytes/s] 1.0E-06*PMC0*64.0/time
Prefetch data volume [GBytes] 1.0E-09*PMC0*64.0

LONG
Formulas:
Prefetch bandwidth [MBytes/s] = 1.0E-06*HWP_L2MISS*64.0/time
Prefetch data volume [GBytes] = 1.0E-09*HWP_L2MISS*64.0
-
The bandwidth and data volume caused by L2 misses from the hardware prefetcher.

