SHORT Memory write bandwidth

EVENTSET
PMC0  L2_VICTIM_REQ_WITH_DATA
PMC1  SNP_HITM_L2


METRICS
Runtime (RDTSC) [s] time
Memory write bandwidth [MBytes/s] 1.0E-06*(PMC0+PMC1)*64.0/time
Memory write data volume [GBytes] 1.0E-09*(PMC0+PMC1)*64.0

LONG
Formulas:
Memory write bandwidth [MBytes/s] = 1.0E-06*(L2_VICTIM_REQ_WITH_DATA+SNP_HITM_L2)*64.0/time
Memory write data volume [GBytes] = 1.0E-09*(L2_VICTIM_REQ_WITH_DATA+SNP_HITM_L2)*64.0
-
Bandwidth and data volume of write operations from the L2 cache to memory. The
metric is introduced in the book 'Intel Xeon Phi Coprocessor High-Performance
Programming' by James Jeffers and James Reinders.
