SHORT L2 read misses

EVENTSET
PMC0  L2_DATA_READ_MISS_MEM_FILL

METRICS
Runtime (RDTSC) [s] time
L2 read bandwidth [MBytes/s] 1.0E-06*PMC0*64.0/time
L2 read data volume [GBytes] 1.0E-09*PMC0*64.0

LONG
Formulas:
L2 read bandwidth [MBytes/s] = 1.0E-06*L2_DATA_READ_MISS_MEM_FILL*64.0/time
L2 read data volume [GBytes] = 1.0E-09*L2_DATA_READ_MISS_MEM_FILL*64.0
-
The data volume and bandwidth caused by read misses in the L2 cache.

