SHORT Memory bandwidth

EVENTSET
PMC0  DATA_READ_MISS_OR_WRITE_MISS
PMC1  DATA_CACHE_LINES_WRITTEN_BACK


METRICS
Runtime (RDTSC) [s] time
Memory bandwidth [MBytes/s] 1.0E-06*(PMC0+PMC1)*64.0/time
Memory data volume [GBytes] 1.0E-09*(PMC0+PMC1)*64.0

LONG
Formulas:
Memory bandwidth [MBytes/s] = 1.0E-06*(DATA_READ_MISS_OR_WRITE_MISS+DATA_CACHE_LINES_WRITTEN_BACK)*64.0/time
Memory data volume [GBytes] = 1.0E-09*(DATA_READ_MISS_OR_WRITE_MISS+DATA_CACHE_LINES_WRITTEN_BACK)*64.0
-
Total memory bandwidth and data volume.
