SHORT Read/Write Events between the ccNUMA nodes

EVENTSET
UPMC0  UNC_CPU_TO_DRAM_LOCAL_TO_4
UPMC1  UNC_CPU_TO_DRAM_LOCAL_TO_5
UPMC2  UNC_CPU_TO_DRAM_LOCAL_TO_6
UPMC3  UNC_CPU_TO_DRAM_LOCAL_TO_7

METRICS
Runtime (RDTSC) [s] time
DRAM read/write local to 4 [MegaEvents/s]  1.0E-06*UPMC0/time
DRAM read/write local to 5 [MegaEvents/s]  1.0E-06*UPMC1/time
DRAM read/write local to 6 [MegaEvents/s]  1.0E-06*UPMC2/time
DRAM read/write local to 7 [MegaEvents/s]  1.0E-06*UPMC3/time

LONG
Formulas:
DRAM read/write local to 4 [MegaEvents/s]  1.0E-06*UNC_CPU_TO_DRAM_LOCAL_TO_4/time
DRAM read/write local to 5 [MegaEvents/s]  1.0E-06*UNC_CPU_TO_DRAM_LOCAL_TO_5/time
DRAM read/write local to 6 [MegaEvents/s]  1.0E-06*UNC_CPU_TO_DRAM_LOCAL_TO_6/time
DRAM read/write local to 7 [MegaEvents/s]  1.0E-06*UNC_CPU_TO_DRAM_LOCAL_TO_7/time
-
Profiling group to measure the traffic from local CPU to the different
DRAM NUMA nodes. This group allows to detect NUMA problems in a threaded
code. You must first determine on which memory domains your code is running.
A code should only have significant traffic to its own memory domain.


