SHORT Load to store ratio

EVENTSET
FIXC0 INSTR_RETIRED_ANY
FIXC1 CPU_CLK_UNHALTED_CORE
FIXC2 CPU_CLK_UNHALTED_REF
PMC0  INST_RETIRED_LOADS
PMC1  INST_RETIRED_STORES

METRICS
Runtime (RDTSC) [s] time
Runtime unhalted [s] FIXC1*inverseClock
Clock [MHz]  1.E-06*(FIXC1/FIXC2)/inverseClock
CPI  FIXC1/FIXC0
Load to store ratio PMC0/PMC1

LONG
Formulas:
Load to store ratio = INST_RETIRED_LOADS/INST_RETIRED_STORES
-
This is a simple metric to determine your load to store ratio.

