SHORT Double Precision MFLOP/s

EVENTSET
PMC0  RETIRED_INSTRUCTIONS
PMC1  CPU_CLOCKS_UNHALTED
PMC2  RETIRED_UOPS
PMC3  RETIRED_FLOPS_DOUBLE_ALL

METRICS
Runtime (RDTSC) [s] time
Runtime unhalted [s]  PMC1*inverseClock
DP MFLOP/s    1.0E-06*(PMC3)/time
CPI   PMC1/PMC0
CPI (based on uops)   PMC1/PMC2
IPC   PMC0/PMC1

LONG
Formulas:
DP MFLOP/s = 1.0E-06*(RETIRED_FLOPS_DOUBLE_ALL)/time
-
Profiling group to measure double precisision FLOP rate.


