SHORT Cache and memory bandwidths

EVENTSET
PMC0  LONGEST_LAT_CACHE_MISS
PMC1  OFFCORE_RESPONSE_1_WB_ANY

METRICS
SUM Memory read bandwidth [MBytes/s] 1.0E-06*(PMC0)*64.0/time
SUM Memory writeback bandwidth [MBytes/s] 1.0E-06*(PMC1)*64.0/time
SUM Memory bandwidth [MBytes/s] 1.0E-06*(PMC0+PMC1)*64.0/time

LONG
